

Vocollect A720 & A710

Mobile Devices

Today’s distribution center (DC) requires solutions that optimize operations and provide business flexibility, while maximizing existing technology investments. That is why Honeywell Vocollect™ voice solutions are the performance choice for more than one million workers around the world each day. Empowering mobile workers to operate hands free with voice technology has been proven to offer positive worker productivity and business value.

*Vocollect A720*

*Mobile Device*

Within the Vocollect A700 Series from Honeywell, the

first-of-its-kind Vocollect A730 mobile device offers combined voice and scanning. Two additional device options within the A700 Series offer customers the best and most cost-effective fit for their particular needs: the Vocollect A720 and A710 mobile devices.

*Vocollect A710*

*Mobile Device*

The Vocollect A720 mobile device has two industrial-grade

breakaway TCO connectors, identical to those used on prior Vocollect devices. This is the best solution for customers who prefer a Vocollect A700 Series solution that includes support for both wireless and wired Vocollect headsets and certified wired peripherals.

Honeywell understands that every customer has unique

requirements for the warehouse and distribution center. Offering a wide choice of device and solution options is yet another example of how Honeywell can help you run a better business with voice.

The Vocollect A710 is a wireless-only device that is the best fit

for voice-only workflows in environments where operators are using Vocollect Bluetooth®-enabled headsets and peripherals. This device is also ideal for vehicle-based workflows.

F E AT URE S

&

BE N E F I T S

Empowering mobile workers to operate hands free with voice technology has been proven to offer positive worker productivity and business value.

With two TCO connectors, the Vocollect A720 mobile device is the best solution for customers who prefer a device with support for both wireless and wired Vocollect headsets and certified wired peripherals.

The Vocollect A710 wireless-only device is the best fit for voice-only workflows in environments where operators

are using Vocollect Bluetooth-enabled headsets and peripherals. This device is also ideal for vehicle-based workflows.

Both devices offer a choice of two battery options: a standard battery, projected to last 14 hours, and an extended life battery, projected to last 24 hours (a nice option for freezer environments). Either choice helps eliminate work stoppage associated with battery changes.

Both devices support a number of time-saving features, including TouchConnect™, TouchConfig™, RapidStart™ and other features designed for faster start-up times, resulting in greater worker productivity.

Vocollect A720 & A710 Technical Specifications

A 72 0

A 7 10

**GENERAL SPECIFICATIONS**

Best Used for:

Environments where a wired long-range scanner or other wired peripherals are required

Supporting wireless headsets and peripherals

**VOCOLLECT VOICE SOFTWARE**

Vocollect VoiceConsole™ 5.0 +

Vocollect VoiceConsole 5.0 +

Device Management Software:

Speech Recognizer:

Vocollect BlueStreak™

Vocollect BlueStreak

**VOCOLLECT DEVICE**

Storage Temperature:

-40°C to 70°C (-40°F to 158°F)

-40°C to 70°C (-40°F to 158°F)

Vibration:

Meets MIL-STD-810F method 514.6

Meets MIL-STD-810F method 514.6

Humidity:

100% condensing

100% condensing

**RADIO**

Bluetooth Version:

Class 2 Bluetooth v2.1 + EDR

Class 2 Bluetooth v2.1 + EDR

**VOCOLLECT HEADSET SUPPORT**

WEIGHT

245 g (8.6 oz)

238 g (8.4 oz)

With Standard Battery:

**SIZE**

For a complete listing of all compliance approvals and certifications, please visit [www.honeywellaidc.com/compliance.](http://www.honeywellaidc.com/compliance) For a complete listing of all supported barcode symbologies, please visit [www.honeywellaidc.com/symbologies.](http://www.honeywellaidc.com/symbologies)

**Honeywell Sensing and**

**Productivity Solutions** 9680 Old Bailes Road Fort Mill, SC 29707

800-582-4263

[www.honeywell.com](http://www.honeywell.com/)

Vocollect A720 & A710 DS Rev B 12/15

© 2015 Honeywell International Inc.

Standard L × H × W: 135.6 mm × 64.1 mm × 42.1 mm 137.9 mm × 64.1 mm × 42.1 mm

(5.3 in × 2.5 in × 1.7 in) (5.4 in × 2.5 in × 1.7 in)

With High-Capacity Battery:

296 g (10.4 oz)

289 g (10.2 oz)

Terminal:

165 g (5.8 oz)

158 g (5.6 oz)

Configurations Supported: Vocollect Wired SR Series Headsets, Vocollect SRX and SRX2 Wireless Headsets

Vocollect SL-14 Headset, Vocollect SRX and SRX2 Wireless Headsets

NFC/Vocollect TouchConnect:

Yes with Vocollect VoiceCatalyst

Yes with Vocollect VoiceCatalyst

Wi-Fi:

802.11a/b/g/n

802.11a/b/g/n

Rain & Dust Sealing:

IP67

IP67

Battery Indication:

Yes

Yes

Drop Tested: 24 drops at 1.5 m (5 ft) to steel; 24 drops at 1.5 m (5 ft) to steel; 12 drops at 1.8 m (6 ft) to steel 12 drops at 1.8 m (6 ft) to steel

Operating Temperature:

-30°C to 50°C (-22°F to 122°F)

-30°C to 50°C (-22°F to 122°F)

Operating System:

Microsoft® Windows® CE 7

Microsoft Windows CE 7

Voice Processes:

VoiceApplications™ / VoiceTasks™

VoiceApplications / VoiceTasks

Terminal Software: Vocollect VoiceCatalyst™ 2.1 + Vocollect VoiceCatalyst 2.0 + /

Vocollect VoiceClient™ 3.9 +

Endcap Description:

Two (TCO) Connector Wired Endcaps

Standard Endcap